3 x QUOTATIONS – TOWN SIGN REPAIR

**Specification of works**

: provide protective boarding for access.

: supply security fencing for duration of works

: Take down existing brick planter to existing foundations.

:Re build in new brickwork to match existing size and height

: remove old timber post from centre of planter.

:excavate new 2 ft deep hole to accommodate new post

:Fit 1 no new 0.250mm by 0.250mm oak post to project out of ground by 12 ft

:ALL RUBBISH CLEARED FROM SITE

**QUOTE 1**

**Price including VAT £3,744.00**

**QUOTE 2**

**Price including VAT £4,242.00**

**QUOTE 3**

**Price including VAT £4,290.00**